**ENIFLOOD 1000s**

|  |  |
| --- | --- |
| Luminous intensity | 30.000 cd |
| Power | 220 W LED (2 x 110W)Complies 1.500/2000W Tungsten |
| Light-Temperature | 3000 K4000 K5000 K |
| Power Supply | 198 to 264 V; 50/60 Hz |
| Kühlung | Fanless / passive Cooling - noiseless |
| Dimensions (B x H x T)With Handle and Yoke | 332 x 300 x 167 mm352 x 390 x 167 mm |
| Net. weight | 5,75 kg |

Specifikations

* Robust metal housing
* Aluminum heat sink with 8 heatpipes
* Fanless
* Cardboard Filter Holder
* Integrated Reflector of high purity aluminium
* Controlling via DMX512-A
* Integrated Cues for rehearsal- and working-light (without a desk)

Scope of delivery

* Power-Supply cable 2,5m with Schuko and Powercon True