**HPZ 115 D**

|  |  |
| --- | --- |
| Beam angle/zoom | adjustable from 16 to 38° |
| Axial luminous intensity | 215.000 cd at 16°  54.000 cd at 38° |
| Reflector | Dichroic cold light glass reflector |
| Socket | GX 9,5 for Tungsten 1.000 or 1.200 W |
| Dimensions  (A x B xC) | 645 x 320 x 475 mm |
| Net. weight | 14kg |

Specification

* 3 zoom lenses and double condenser optics
* All lenses equipped with broadband anti-reflective coating
* Aspherical condenser lens
* Plano convex intermediate lens in lamp housing
* Convection cooling without fan, without forced ventilation of the lamp, without disturbing fan noise
* Rotatable integrated four-blade shutter and a field-replaceable beam size iris.
* Soft glass mounting option inside the zoom tube
* uniform light distribution with a precise image of the beam shapers and projections
* Focal length and focusing single-side-adjustable by individual controls, to avoid dangers without having to change
* Operating panel with 4-Shaper-Unit and a slot for a gobo holder (size A)
* Optional non-thermoconductive goboholder
* Beam Shaper Unit with 4 non-thermoconductive handles, arranged in 4 levels. With the possibility simultaneously sliding in all 4 shapers
* The lamp housing is fully rotatable through 360° and lockable in its normal orientation.
* Lamp housing cover can be swivelled back to provide rapid access to lamp
* anthracite-coloured heat and wear resistant finish.
* three-slot front cassette according to DIN 15560 (185 x 185mm) for gel holders and accessories
* All metal parts are corrosion-protected.
* Handles and controls are made from non-thermoconductive materials.
* Gobo holder Size A + / - 42° rotatable
* Beam shaping shutters + / - 42° rotatable
* Beam shaping shutters 4 shutters with non-thermoconductive handles, optional 8 shutters
* Endless 360° rotatable and 9-times-lockable lamphouse

Scope of delivery

* Zoom profile spotlight with condenser
* 2.5m main cable Black Colour with assembled Schuko plug (CEE 7/4, Type F).
* Metal protective grid